IFC building model
Schema: "IFC4"
Description: "IFC4"
File name: "construction"
Time stamp: "2026-06-08T11:11:23"
Application: "WinDoPlan planner" version "1.0" identifier "WinDoPlan" by Organization "VEKA AG"

People and organizations
  Person "WinDoPlan" of Organization "VEKA AG"
  Owner history of Person "WinDoPlan" of Organization "VEKA AG" | application "WinDoPlan planner" version "1.0" identifier "WinDoPlan" by Organization "VEKA AG" | change ADDED | created 1780909883 (2026-06-08T09:11:23Z)

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "WinDoPlan" | description "configurator export"
  IFCBUILDING "Default Building" | description "Description of Default Building"
    contains 1 element
      1 x IFCWINDOW | type IFCWINDOWTYPE "SOFTLINE 76 AD 1370x2230mm 2-piece window" | names: "SOFTLINE 76 AD 1370x2230mm 2-piece window" | descriptions: "VEKA AG SOFTLINE 76 AD 1370x2230mm 2-piece window" | property sets: Pset_WindowCommon, Pset_DoorWindowGlazingType, Pset_UserIfcWindow

Types
  IFCWINDOWTYPE "SOFTLINE 76 AD 1370x2230mm 2-piece window" | WINDOW | DOUBLE_PANEL_HORIZONTAL | 1 occurrence | property sets: panel1, panel2 | description "SOFTLINE 76 AD 1370x2230mm 2-piece window"

Property sets
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0.92167 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorWindowGlazingType | properties | on 1 object (1 IFCWINDOW)
    GlassLayers = 3.00000 (IFCCOUNTMEASURE)
  Pset_UserIfcWindow | properties | on 1 object (1 IFCWINDOW)
    Classification = "B3-5-2" (IFCTEXT)
    Manufacturer = "VEKA AG" (IFCTEXT)
    Material = "PVC" (IFCTEXT)
    Profile system = "SOFTLINE 76 AD" (IFCTEXT)
    Profile system depth = "76 mm" (IFCTEXT)
    U-value construction = "0.92167 W/(m2*K)" (IFCTEXT)
    Weight construction = "130 kg" (IFCTEXT)
  panel1 | predefined | on 1 type object
  panel2 | predefined | on 1 type object